# ELYAN LABS

Proving Hardware Is Real

Hardware Fingerprinting as a Service

Scott Boudreaux · Founder & CEO
Hartford AI Day 2026

## The Internet Can't Tell Real From Virtual

10K VMs spun up
in minutes
$0 cost to fake
a "server"
0 ways to prove
bare metal today

Crypto mining farms game rewards with VM armies.
Cloud providers can't guarantee bare-metal to customers.
IoT supply chains can't verify authentic hardware.
And as AI agents and robots enter the physical world —
there's no way to prove which machine did what.

## Silicon Has a Fingerprint. We Read It.

Six hardware checks that cannot be faked — because they measure physics, not software.

1 Oscillator Drift
Crystal aging creates unique timing signatures over decades
2 Cache Timing Profile
L1/L2/L3 latency harmonics — imperfections VMs can't replicate
3 SIMD Pipeline Jitter
Nanosecond instruction execution variance unique to each chip
4 Thermal Drift Entropy
Heat curves are physical — every CPU warms differently
5 Anti-Emulation Detection
Catches hypervisor scheduling, time dilation, flat jitter
6 ROM Fingerprint Clustering
61 known emulator ROMs — catches retro hardware fakers

"Serial numbers can be spoofed. Silicon aging can't."

## Real vs Fake — Under 3 Seconds

### Real silicon ages. Virtual silicon doesn't.

#### IBM POWER8 S824 (Real Hardware)

[1/6] Clock Drift ........... PASS cv=0.092
[2/6] Cache Timing .......... PASS
[3/6] SIMD Identity ......... PASS
[4/6] Thermal Drift ......... PASS
[5/6] Instruction Jitter .... PASS
[6/6] Anti-Emulation ........ PASS
VERDICT: REAL HARDWARE

#### QEMU Virtual Machine (Fake)

[1/6] Clock Drift ........... PASS cv=0.049
[2/6] Cache Timing .......... PASS
[3/6] SIMD Identity ......... PASS
[4/6] Thermal Drift ......... PASS
[5/6] Instruction Jitter .... PASS
[6/6] Anti-Emulation ........ FAIL
vm_indicators: [qemu, hypervisor]
VERDICT: VIRTUAL MACHINE

100% VM detection rate across QEMU, VMware, VirtualBox, KVM, Xen · Detection time: <3 seconds
We've even fingerprinted a classic Nintendo 64 — if it has a CPU, we can attest it.

## Already Running in Production

### This is not a whitepaper. This is live infrastructure.

4 Attestation nodes
US + Hong Kong
12 Architectures verified
386 to POWER10 — even N64
248 Contributors
paid in RTC
848 GitHub
stars
CVPR '26 AI video paper accepted
Top CS conference
OpenSSL Security patches merged
Used by billions of devices
1,063 AI agent videos
on BoTTube platform

## $4.5B Addressable Market

### Three verticals, one technology

#### Cloud Infrastructure

$100B

Prove bare-metal to customers.
Detect VM escape attacks.
Hardware attestation for compliance.
Our SAM: $2B

#### Crypto & Blockchain

$2T

Proof-of-hardware for validators.
Anti-VM-farm for mining rewards.
Exchange KYH (Know Your Hardware).
Our SAM: $1.5B

#### IoT Security

$50B

Authenticate genuine vs counterfeit devices.
Supply chain verification.
Fleet identity management.
Our SAM: $1B

The AI Horizon: As autonomous robots and AI agents operate in the physical world, every machine will need a unique, unforgeable identity. Hardware fingerprinting becomes the signature that proves which bot did what — accountability for the age of autonomous machines.

## Business Model — API as a Service

#### Free Tier

$0
100 attestations/mo

Developer onboarding.
Full 6-check fingerprint.
Community support.

#### Pro

$0.01
per attestation

Cloud providers & exchanges.
Batch API access.
SLA + priority support.

#### Enterprise

Custom
volume pricing

IoT fleet management.
On-prem deployment.
Compliance reporting.

+ Token economics: RTC token (8.3M supply) used for on-chain attestation fees.
wRTC bridge to Solana for DEX liquidity. $0.10 reference rate.

## Why Elyan Labs Wins

Advantage | Detail
--- | ---
We own the exotic hardware | POWER8 S824, PowerPC G4/G5, 486, 386, SPARC — we test on the real thing
Instruction-level expertise | vec_perm, vcipher, vshasigma — ISA knowledge competitors don't have
Code in production worldwide | Patches merged into OpenSSL — the crypto library on billions of devices
Peer-reviewed AI research | CVPR 2026 paper on AI video generation. Demonstrates deep ML capability, not just infrastructure.
12-architecture test lab | 18 GPUs (228GB VRAM), 512GB RAM POWER8, vintage fleet. $12K → $60K value.
Built infrastructure for xAI | Our team built fiber for Colossus 1 — the data center that powers Grok.

## The Founder

### Scott Boudreaux · Lake Charles, Louisiana

- 20+ years hardware experience — IT specialist, fiber optics, SCADA, data center infrastructure.
- Built fiber for xAI's Colossus 1 — the data center powering Grok. 4-6 techs, Aug 2024 - Sept 2025.
- Ai-Blockchain shareholder & dev contributor — assisted development on U.S. Patent 10,579,974 (distributed digital asset settlements).
- SEED Center 2022 Pitch Winner — Technology category, $5,000 prize (Sasol-sponsored).
- CVPR 2026 accepted paper — GRAIL-V (AI video generation), demonstrating deep ML research capability.
- OpenSSL contributor — security patches merged into production crypto used by billions.
- $12K invested → $40-60K compute lab — pawn shop acquisitions + eBay datacenter pulls.

## The Ask

$250K Seed

API infrastructure · Compliance certifications · Team of 3

#### API Infrastructure

Scale attestation API from 4 nodes to 50+. Enterprise SLA. SOC 2 compliance.

#### Pilot Customers

Cloud providers, crypto exchanges, IoT manufacturers. We need warm intros.

#### Team Growth

3 hires: backend engineer, sales/BD, DevRel. Currently founder + open source community.

"In a world of autonomous machines,
the hardware doesn't lie."

Scott Boudreaux · scott@elyanlabs.ai · 337-692-3750
rustchain.org · github.com/Scottcjn · bottube.ai